The relay has 2 potential-free contacts. The maximum power specified below can be switched for each contact. Furthermore, both contacts can be controlled independently of one another. With the additional "Long Range" feature, you can now enjoy reliable control even from greater distances.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output voltage AC max.: 250 V

Output voltage DC max.: 25 V

Output max.: 1.500 VA

Switching output: 1.500 VA

Acceptance tests:

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 143 mm

Width (B): 38 mm

Height (H): 23 mm

Manufacturer: RP-Technik GmbH