The CASA ROLLO roller shutter control system can be used to control or operate roller shutters, blinds or awnings via a push button or app.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output max.: 345 VA

Switching output: 345 VA

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 143 mm

Width (B): 38 mm

Height (H): 27 mm

Manufacturer: RP-Technik GmbH