The CO-TED460W-01 is a CASAMBI® trailing edge controller. This enables continuous dimming via the CASAMBI® app. The controller is designed for an input voltage of 120-277 VAC and max. 2A and can supply a power consumption of up to 460W.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output max.: 460 W

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 101,2 mm

Width (B): 51,1 mm

Height (H): 24 mm

Manufacturer: RP-Technik GmbH