LED recessed luminaire, frame panel, EDGE series, for 625 mm ceiling module. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply, can be switched or dimmed (DALI/TRIAC dimmer), external. Version with CASAMBI® Bluetooth control, RGBW and tunable white available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 40 W

Photometrical data:

Rated luminous flux: 1.350 lm

Colour temperature: K

Light source: LED

Physical data:

Length (L): 615 mm

Width (B): 615 mm

Height (H): 15 mm

Ceiling Cut-out L: 0 mm

Ceiling Cut-out W: 0 mm

Manufacturer: RP-Technik GmbH