LED recessed surface-mounted luminaire, LINDO series, IP65, for use in places with stringent requirements (hospitals, laboratories, operating theatres, food industry etc.). Housing made from steel plate, powder-coated. Diffuser made from PMMA, UV-resistant. Power supply, can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible. NANO protection on request.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 65

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 50 W

Photometrical data:

Rated luminous flux: 4.250 lm

Colour temperature: 3000 K

UGR: 20.9

Light source: LED

Physical data:

Length (L): 1.090 mm

Width (B): 355 mm

Height (H): 87 mm

Manufacturer: RP-Technik GmbH