LED recessed luminaire, VARIO series, 2700K-6500K tunable white. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply can be dimmed, external. UGR 19 and screen-compliant in accordance with EN 12464-1. Version with CASAMBI® Bluetooth control.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 24 W

Photometrical data:

Rated luminous flux: 1.800 lm

Colour temperature: 2700-6500 K

Light source: LED

Physical data:

Length (L): 295 mm

Width (B): 295 mm

Height (H): 10 mm

Manufacturer: RP-Technik GmbH