LED luminaire, RGBW series. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply can be dimmed, external. Version with CASAMBI® Bluetooth control.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 9 W

Photometrical data:

Rated luminous flux: lm

Colour temperature: K

Light source: LED

Physical data:

Length (L): 180 mm

Width (B): 180 mm

Height (H): 10 mm

Manufacturer: RP-Technik GmbH