LED panel "VARIO" for ceiling recessed mounting, RGBW series. Flat design. Aluminum frame, white, powder coated. Diffuser made of synthetic material (PMMA), opal, non-yellowing. Power supply dimmable, external. Version with Casambi Bluetooth control.

Acceptance tests:

Electrical data:

System power: 54 W

Photometrical data:

Rated luminous flux: lm

Physical data:

Length (L): 620 mm

Width (B): 620 mm

Height (H): 10 mm

Manufacturer: RP-Technik GmbH