Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 35 W

Photometrical data:

Rated luminous flux: 4.600 lm

Colour temperature: 4000 K

UGR: 18

Light source: LED

Physical data:

Length (L): 1.403 mm

Width (B): 93 mm

Height (H): 80 mm

Ceiling Cut-out L: mm

Ceiling Cut-out W: mm

Ceiling Cut-out ø: mm

Producent RP-Technik GmbH