LED ceiling- and wall-mounted luminaire, MAVS. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with  
CASAMBI® Bluetooth control available. DC compatible.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 26 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 2.750 lm

Colour temperature: 4000 K

UGR: 26.2

Light source: LED

Physical data:

Length (L): 850 mm

Width (B): 59 mm

Height (H): 79 mm

Manufacturer: RP-Technik GmbH