LED ceiling- and wall-mounted luminaire, RONDO series, with direct/indirect beam, as the basic lighting for rooms in a commercial environment and at home. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 28 W

DC Ready: Yes

Rated power: W

Photometrical data:

Rated luminous flux: 3.350 lm

Colour temperature: 3000 K

UGR: 23.9

Light source: LED

Physical data:

Height (H): 62 mm

Diameter ø: 400 mm

Manufacturer: RP-Technik GmbH