LED ceiling- and wall-mounted luminaire, RONDO series, with direct/indirect beam, as the basic lighting for rooms in a commercial environment and at home. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI Bluetooth control available. DC compatible.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 16 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 2.100 lm

Colour temperature: 4000 K

UGR: 22.1

Light source: LED

Physical data:

Height (H): 62 mm

Diameter ø: 400 mm

Manufacturer: RP-Technik GmbH