Flexible parallel bracket, which allows the entire luminaire housing to be aligned. The bracket can be used, for example, to align safety luminaires to optimise illumination of escape and emergency routes. 

Brand: RP-Technik GmbH
