Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 33 W

Photometrical data:

Rated luminous flux: 3.450 lm

Colour temperature: 3000 K

Light source: LED

Physical data:

Length (L): 1.122 mm

Width (B): 93 mm

Height (H): 80 mm

Producent RP-Technik GmbH