Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 31 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 4.150 lm

Colour temperature: 4000 K

UGR: 14.4

Light source: LED

Physical data:

Length (L): 1.135 mm

Width (B): 50 mm

Height (H): 125 mm

Producent RP-Technik GmbH