Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 63 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 7.250 lm

Colour temperature: 3000 K

UGR: 12

Light source: LED

Physical data:

Length (L): 1.415 mm

Width (B): 50 mm

Height (H): 125 mm

Producent RP-Technik GmbH